Unit Name:                  IPD1200     

Preset Name:            SUB120 300W     
Preset Number:          17

Input 1
Channel Name:                     
Gain:              0.0dB
Mute:              Off
Invert:            Off
Stereo Link:       On
Mixer Input 3:     0.0dB
Mixer Input 4:     -48.0dB
Mixer Input 1:     0.0dB
Mixer Input 2:     -48.0dB
Delay:             0.0ms
HPF Frequency:     Off
HPF Type:          24dB Linkwitz-Riley
HPF Enable:        On
LPF Frequency:     Off
LPF Type:          24dB Linkwitz-Riley
LPF Enable:        On
PEQ 1 Gain:        0.0dB
PEQ 1 Frequency:   20.0Hz
PEQ 1 Q:           1.0
PEQ 1 Type:        Bell
PEQ Enable:        Off
PEQ 2 Gain:        0.0dB
PEQ 2 Frequency:   40.0Hz
PEQ 2 Q:           1.0
PEQ 2 Type:        Bell
PEQ Enable:        Off
PEQ 3 Gain:        0.0dB
PEQ 3 Frequency:   80.0Hz
PEQ 3 Q:           1.0
PEQ 3 Type:        Bell
PEQ Enable:        Off
PEQ 4 Gain:        0.0dB
PEQ 4 Frequency:   160.0Hz
PEQ 4 Q:           1.0
PEQ 4 Type:        Bell
PEQ Enable:        Off
PEQ 5 Gain:        0.0dB
PEQ 5 Frequency:   320.0Hz
PEQ 5 Q:           1.0
PEQ 5 Type:        Bell
PEQ Enable:        Off
PEQ 6 Gain:        0.0dB
PEQ 6 Frequency:   640.0Hz
PEQ 6 Q:           1.0
PEQ 6 Type:        Bell
PEQ Enable:        Off
PEQ 7 Gain:        0.0dB
PEQ 7 Frequency:   1280.0Hz
PEQ 7 Q:           1.0
PEQ 7 Type:        Bell
PEQ Enable:        Off
PEQ 8 Gain:        0.0dB
PEQ 8 Frequency:   2560.0Hz
PEQ 8 Q:           1.0
PEQ 8 Type:        Bell
PEQ Enable:        Off
PEQ 9 Gain:        0.0dB
PEQ 9 Frequency:   5120.0Hz
PEQ 9 Q:           1.0
PEQ 9 Type:        Bell
PEQ Enable:        Off
PEQ 10 Gain:       0.0dB
PEQ 10 Frequency:  10240.0Hz
PEQ 10 Q:          1.0
PEQ 10 Type:       Bell
PEQ Enable:        Off
Limiter Release:   50.0dB/s
Compressor Makeup Gain:   0.0sB
Compressor Threshold: 37.82dBu
Compressor Attack:   20.0ms
Compressor Release:  50.0ms
Compressor Hold:     10.0ms
Compressor Ratio:   1:2.0

Input 2
Channel Name:                     
Gain:              0.0dB
Mute:              Off
Invert:            Off
Mixer Input 2:     0.0dB
Mixer Input 1:     -48.0dB
Mixer Input 3:     -48.0dB
Mixer Input 4:     0.0dB
Delay:             0.0ms
HPF Frequency:     Off
HPF Type:          24dB Linkwitz-Riley
HPF Enable:        On
LPF Frequency:     Off
LPF Type:          24dB Linkwitz-Riley
LPF Enable:        On
PEQ 1 Gain:        0.0dB
PEQ 1 Frequency:   20.0Hz
PEQ 1 Q:           1.0
PEQ 1 Type:        Bell
PEQ Enable:        Off
PEQ 2 Gain:        0.0dB
PEQ 2 Frequency:   40.0Hz
PEQ 2 Q:           1.0
PEQ 2 Type:        Bell
PEQ Enable:        Off
PEQ 3 Gain:        0.0dB
PEQ 3 Frequency:   80.0Hz
PEQ 3 Q:           1.0
PEQ 3 Type:        Bell
PEQ Enable:        Off
PEQ 4 Gain:        0.0dB
PEQ 4 Frequency:   160.0Hz
PEQ 4 Q:           1.0
PEQ 4 Type:        Bell
PEQ Enable:        Off
PEQ 5 Gain:        0.0dB
PEQ 5 Frequency:   320.0Hz
PEQ 5 Q:           1.0
PEQ 5 Type:        Bell
PEQ Enable:        Off
PEQ 6 Gain:        0.0dB
PEQ 6 Frequency:   640.0Hz
PEQ 6 Q:           1.0
PEQ 6 Type:        Bell
PEQ Enable:        Off
PEQ 7 Gain:        0.0dB
PEQ 7 Frequency:   1280.0Hz
PEQ 7 Q:           1.0
PEQ 7 Type:        Bell
PEQ Enable:        Off
PEQ 8 Gain:        0.0dB
PEQ 8 Frequency:   2560.0Hz
PEQ 8 Q:           1.0
PEQ 8 Type:        Bell
PEQ Enable:        Off
PEQ 9 Gain:        0.0dB
PEQ 9 Frequency:   5120.0Hz
PEQ 9 Q:           1.0
PEQ 9 Type:        Bell
PEQ Enable:        Off
PEQ 10 Gain:       0.0dB
PEQ 10 Frequency:  10240.0Hz
PEQ 10 Q:          1.0
PEQ 10 Type:       Bell
PEQ Enable:        Off
Limiter Release:   50.0dB/s
Compressor Makeup Gain:   0.0sB
Compressor Threshold: 37.82dBu
Compressor Attack:   20.0ms
Compressor Release:  50.0ms
Compressor Hold:     10.0ms
Compressor Ratio:   1:2.0

Input 3

Input 4

Input 5

Output 1
Channel Name:     SUB OUT         
Gain:              4.0dB
Mute:              On
Invert:            Off
Stereo Link:       On
Delay:             0.0ms
HPF Frequency:     30.0Hz
HPF Type:          18dB Butterworth
HPF Enable:        On
LPF Frequency:     120.0Hz
LPF Type:          24dB Linkwitz-Riley
LPF Enable:        On
PEQ 1 Gain:        0.0dB
PEQ 1 Frequency:   20.0Hz
PEQ 1 Q:           1.0
PEQ 1 Type:        Bell
PEQ Enable:        Off
PEQ 2 Gain:        0.0dB
PEQ 2 Frequency:   37.0Hz
PEQ 2 Q:           2.9
PEQ 2 Type:        Bell
PEQ Enable:        Off
PEQ 3 Gain:        3.0dB
PEQ 3 Frequency:   40.0Hz
PEQ 3 Q:           3.6
PEQ 3 Type:        Bell
PEQ Enable:        On
PEQ 4 Gain:        0.0dB
PEQ 4 Frequency:   160.0Hz
PEQ 4 Q:           1.0
PEQ 4 Type:        Bell
PEQ Enable:        Off
PEQ 5 Gain:        0.0dB
PEQ 5 Frequency:   320.0Hz
PEQ 5 Q:           1.0
PEQ 5 Type:        Bell
PEQ Enable:        Off
PEQ 6 Gain:        0.0dB
PEQ 6 Frequency:   2144.0Hz
PEQ 6 Q:           2.6
PEQ 6 Type:        Bell
PEQ Enable:        Off
PEQ 7 Gain:        0.0dB
PEQ 7 Frequency:   1280.0Hz
PEQ 7 Q:           1.0
PEQ 7 Type:        Bell
PEQ Enable:        Off
PEQ 8 Gain:        0.0dB
PEQ 8 Frequency:   2560.0Hz
PEQ 8 Q:           1.0
PEQ 8 Type:        Bell
PEQ Enable:        Off
PEQ 9 Gain:        0.0dB
PEQ 9 Frequency:   5120.0Hz
PEQ 9 Q:           1.0
PEQ 9 Type:        Bell
PEQ Enable:        Off
PEQ 10 Gain:       -2.5dB
PEQ 10 Frequency:  20000.0Hz
PEQ 10 Q:          12.0
PEQ 10 Type:       High Shelf
PEQ Enable:        On
Limiter Threshold: 33.8dBu
Limiter Release:   50.0dB/s
Compressor Makeup Gain:   0.0sB
Compressor Threshold: 33.78dBu
Compressor Attack:   20.0ms
Compressor Release:  50.0ms
Compressor Hold:     10.0ms
Compressor Ratio:   1:2.0

Output 2
Channel Name:     SUB OUT         
Gain:              4.0dB
Mute:              On
Invert:            Off
Delay:             0.0ms
HPF Frequency:     30.0Hz
HPF Type:          18dB Butterworth
HPF Enable:        On
LPF Frequency:     120.0Hz
LPF Type:          24dB Linkwitz-Riley
LPF Enable:        On
PEQ 1 Gain:        0.0dB
PEQ 1 Frequency:   20.0Hz
PEQ 1 Q:           1.0
PEQ 1 Type:        Bell
PEQ Enable:        Off
PEQ 2 Gain:        0.0dB
PEQ 2 Frequency:   37.0Hz
PEQ 2 Q:           2.9
PEQ 2 Type:        Bell
PEQ Enable:        Off
PEQ 3 Gain:        3.0dB
PEQ 3 Frequency:   40.0Hz
PEQ 3 Q:           3.6
PEQ 3 Type:        Bell
PEQ Enable:        On
PEQ 4 Gain:        0.0dB
PEQ 4 Frequency:   160.0Hz
PEQ 4 Q:           1.0
PEQ 4 Type:        Bell
PEQ Enable:        Off
PEQ 5 Gain:        0.0dB
PEQ 5 Frequency:   320.0Hz
PEQ 5 Q:           1.0
PEQ 5 Type:        Bell
PEQ Enable:        Off
PEQ 6 Gain:        0.0dB
PEQ 6 Frequency:   2144.0Hz
PEQ 6 Q:           2.6
PEQ 6 Type:        Bell
PEQ Enable:        Off
PEQ 7 Gain:        0.0dB
PEQ 7 Frequency:   1280.0Hz
PEQ 7 Q:           1.0
PEQ 7 Type:        Bell
PEQ Enable:        Off
PEQ 8 Gain:        0.0dB
PEQ 8 Frequency:   2560.0Hz
PEQ 8 Q:           1.0
PEQ 8 Type:        Bell
PEQ Enable:        Off
PEQ 9 Gain:        0.0dB
PEQ 9 Frequency:   5120.0Hz
PEQ 9 Q:           1.0
PEQ 9 Type:        Bell
PEQ Enable:        Off
PEQ 10 Gain:       -2.5dB
PEQ 10 Frequency:  20000.0Hz
PEQ 10 Q:          12.0
PEQ 10 Type:       High Shelf
PEQ Enable:        On
Limiter Threshold: 33.8dBu
Limiter Release:   50.0dB/s
Compressor Makeup Gain:   0.0sB
Compressor Threshold: 33.78dBu
Compressor Attack:   20.0ms
Compressor Release:  50.0ms
Compressor Hold:     10.0ms
Compressor Ratio:   1:2.0


Other:
