X-TOUCH Editor 
--------------
Windows editor for X-TOUCH COMPACT and X-TOUCH MINI, supporting Windows 7 and above.

The editor is required for...
1. Changing controller assignments 
2. Save/load presets (layers)
3. Updating firmware



This release version contains:
------------------------------
1. X-TOUCH Editor v1.21

2. Update Files:
Firmware v1.14 for X-TOUCH COMPACT 
For X-TOUCH MINI there is no update.

3. Default Layers:
Layers A + B (factory settings) for X-TOUCH COMPACT
Layers A + B (factory settings) for X-TOUCH MINI


IMPORTANT NOTE:
All operations (edit, firmware update, factory reset) are handled within the editor.


Generally there is no need to update the firmware or to reload factory presets.
If you notice any problems, please visit www.behringer.com for updates.



Editor operation - quick introduction:
---------------------------------------
- Download the editor from www.behringer.com

- Unzip to the desired location (e.g. programs folder or desktop)

- Open the "X-TOUCH EDITOR" folder

- Double-click on the X-TOUCH application to start the editor

- If no hardware is connected, the editor starts in "Dummy mode":
  > "Compact" or "Mini" can be manually selected on the GLOBAL page.
  > All control elements can be edited offline and saved to computer, without the need for connected hardware.

- If any hardware is connected, the editor will automatically detect the correct model and firmware.

- If more than one hardware unit is connected, the preferred unit can be easily selected under "Hardware."
  Note: Several units can be connected simultaneously (e.g. 1x COMPACT, 2x MINI).


- To start editing, there are 3 options:
  1. LOAD a preset from the computer
  2. GET Layer A or B from the connected hardware (this will dump the selected preset into the editor)
  3. Just start from scratch, going through all tabs to make the desired settings


- After editing, there are two options: 
  (The preset has to be saved or dumped)
  1. SAVE to computer
  2. DUMP to the desired layer location A or B on the connected hardware



Factory Reset (loading the default layers):
-------------------------------------------
Option 1:
- Power off the unit (for X-TOUCH MINI: disconnect from USB)
- Hold down both LAYER A/B buttons
- Power on the unit (for X-TOUCH MINI: reconnect USB to computer)
- Wait approximately 10 seconds until the LEDs stop blinking
- Release both LAYER buttons

Option 2:
- Power on / connect the unit to a Windows computer
- Start the X-TOUCH editor
- Press "Load" button
- Open "default layer" folder
- Open the sub folder with the name of your hardware (e.g. "mini" for X-TOUCH MINI)
- Load Layer A (or B)
- Press "Dump A" (or "Dump B") to send the default preset to your hardware



Updating the firmware of the X-TOUCH COMPACT:
---------------------------------------------
Prepare the X-Touch:

Power off the X-Touch by disconnecting the USB cable from the device.
Enter Firmware Update Mode:

Press and hold down the two left buttons of the upper middle row (the "MC" button and the neighboring button).
While holding these buttons, reconnect the USB cable to your Windows computer. This will power on the unit and enter firmware update mode.
Wait for Initialization:

Wait approximately 10 seconds until the LEDs on the X-Touch stop blinking.
Release Buttons:

Release both buttons after the LEDs have stabilized.
Start the X-Touch Editor:

Open the X-Touch Editor application on your Windows PC.
Check Firmware Detection:

In the X-Touch Editor, check if your hardware is detected in the bottom area. The firmware version should display as: N/A.
Update Firmware:

Press the "Update" button in the X-Touch Editor.
The latest firmware is already included in the "Update Files" Folder and pressing "Update" in the X-Touch Editor will automatically find and start the update.
Wait for the update process to complete. This may take a few minutes.
Verify Update:

Once the update is complete, verify that the newly-loaded firmware version is shown in the bottom area of the X-Touch Editor.


Updating the firmware of the X-TOUCH MINI:
------------------------------------------
Prepare the X-Touch:

Power off the X-Touch by disconnecting the USB cable from the device.
Enter Firmware Update Mode:

Press and hold down the two left buttons of the lower row (the "MC" button and the neighboring button).
While holding these buttons, reconnect the USB cable to your Windows computer. This will power on the unit and enter firmware update mode.
Wait for Initialization:

Wait approximately 10 seconds until the LEDs on the X-Touch stop blinking.
Release Buttons:

Release both buttons after the LEDs have stabilized.
Start the X-Touch Editor:

Open the X-Touch Editor application on your Windows PC.
Check Firmware Detection:

In the X-Touch Editor, check if your hardware is detected in the bottom area. The firmware version should display as: N/A.
Update Firmware:

Press the "Update" button in the X-Touch Editor.
The latest firmware is already included in the "Update Files" Folder and pressing "Update" in the X-Touch Editor will automatically find and start the update.
Wait for the update process to complete. This may take a few minutes.
Verify Update:

Once the update is complete, verify that the newly-loaded firmware version is shown in the bottom area of the X-Touch Editor.



