Lake XP preset for ADAMSON IS10n
=========================

Application Notes:
     - Default tuning for 7 to 11 cabinets per array. Use Array Shaping Overlay for different array length and/or to adjust LF contour
     - Array Shaping Overlay must be recalled in a group assigned to all modules of the array
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 3 / 1 with pin swap cable
     - Module out 2 - HF: Ch. 4 / 2 with pin swap cable

Technical Info:
     - Fingerprint: V3.0

=======================
Designed by ADAMSON & DV2
