Lake preset for MDC-2 SUB

Application Notes:
     The preset is low-passed at 80 Hz
     Delay and gain adjusted to match SECTOR C2 Xo85
	To be used with 2xMDC2 + 2xSECTOR
	
Routing MDC2
     SUB : 1+1-
     OUTPUT to crosslink SUB2 : 2 

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2

