EV's PLM Series preset suitable for EV's PHOENIX PX1122M.

EV PX1122M in 2w Bi-Amp mode to be used as floor monitor.

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.

EV Rev Number: Version 2.0 (Standart Preset IIR/DX38)
Dolby Lake Rev Number: Version 1.0

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 148 Vpk (LF), 78 Vpk (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)