EV's PLM Series preset suitable for EV's XLC system.

Application Notes:
Xlc 127+ with Xlc 118 in 4-way mode

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 130 Vpk (SUB), 98 Vpk (LF), 80 Vpk (MF), 69.1 Vpk (HF)
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)