Adamson's PLM Series preset for Adamson's LX12 + B118

Application Notes:
     Passive Mode
     FOH position  
     Setting for 2 LX12 per channel.

Routing:
     LX12 : 1+ 1-
     B118 : 1+ 1-
     Need Extra Audio Panel

Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME