Lake preset for ADAMSON E218
========================

Application Notes:
     - Front-Back (bottom sub forward direction) cardioid configuration
     - Linear Phase Latency included
     - Low passed at 100 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - Front: Ch. 1 / 2
     - Module out 2 -  Back: Ch. 3 / 4 (Use output connector) 

Technical Info:
     - Fingerprint: V2.0

=======================
Designed by ADAMSON & DV2