TURBOSOUND's NuQ102 CUT Bi-Amped FIR preset + NuQ115B SUB

This preset is for FOH applications.

As this is an FIR preset, two modules of processing are required (A+B or C+D) and this preset is not compatible with LM series processors.

Application notes:

Channel 1 = NuQ115B SUB
Channel 2 = NuQ102 LF
Channel 3 = NuQ102 HF

HPF on LF channel is at 100Hz for use with NuQ115B

Total Processor Delay is 6.35ms

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at 3 dBu (SUB), 0.7 dBu (LF), -10.5 dBu (HF)
* MaxPeak limiter threshold at 9 dBu (SUB), 6.7 dBu (LF), -4.5 dBu (HF)
* ISVPL threshold at 89 Vpk (SUB), 69 Vpk (LF), 19 Vpk (HF)  

**Designed by MUSIC TRIBE BRANDS Ltd 2019**
