EAW's PLM Series preset for EAW's JFL speaker.

JFL210x1 Single-amp "Near" w/ Sub High Pass Filter

Application Notes:
JFL210 is high-passed at 100 Hz with 24 dB Linkwitz-Riley filter for 
use with subwoofer. Use for front or side fill applications where 
typical listener distances are <2 meters. Set HF Shading switch to "Single Box".

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.