Adamson's PLM Series preset for Adamson's SpekTrix speaker.

Application Notes:
     The preset is high-passed at 90 Hz
     Maximum of 4 cabinets in parallel per amplifier.

Routing:
     Ch1 : Free
     LF : 2
     MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     SpekTrix v1.0b BETA
     Beta fingerprints may produce incorrect results

Designed by DV2
Pascal GUILLAUME