Lab.gruppen's PLM Series preset suitable for L-Acoustics' X12 full range monitorspeaker, with optional SB18 sub output. V5.8

Application notes:
The module file is a one-way configuration, high-passed at 50 Hz on output 2. 
SB18 is on output 1. Output 3 is an Aux output.
The X12 filter is IIR for shortest latency of 1.71 ms.(Compared to L-Acoustics' 0.76 ms.)
Delay range is 0 - 20ms for both enclosures for flexible placement

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +6 dBu (X12), 9 dBu (SB18)
* ISVPL threshold at 140 Vpk (X12), 117 Vpk (SB18)
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +19 dBu-pk (X12), +16 dBu-pk (SB18)

