Adamson's PLM Series preset for Adamson's Y18 and Y10K

Application Notes:
     This module was designed to be used as a supermodule
     The preset is high-passed at 60 Hz

Routing:
     Y18 LF : 1 & 2
     Y18 MF : 3
     Y18 HF : 4
     Y10K LF : 1 & 2
     Y10K MF : 3
     Y10K HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME