RX599
5.25 inch Coaxial Loudspeaker (Single-amp)
90 x 90 degree nominal beamwidth

Application Notes:
Use for 70 V applications.
Pre-Out EQ tab has user-adjustable high pass filter. Set it no lower than 80 Hz, 24 dB Linkwitz-Riley for full range operation.

Technical info:
* Amplifier Gain is set to 32 dB.
* Factory ISVPL Speaker Thresholds and MaxRMS Limiter Thresholds are engaged.