Lab.gruppen's PLM Series preset suitable for L-Acoustics' KUDO speaker.

Application notes:
In use, route channel LF to two separate amplifier outputs, driving 
one LF driver each, high-passed at 60 Hz.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (LF), +7 dBu (MF), +4 dBu (HF)
* ISVPL threshold at 137.8 Vpk (LF), 122.8 Vpk (MF), 87.0 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (LF), +12 dBu-pk (MF), +9 dBu-pk (HF)

Fingerprint info:
KUDO v1.0b2
Approved ambient temperature range +12 - +50 degrees Celsius