

*****TURBOSOUND TFA-600H SUITABLE FOR FLASHLINE UNDERHUNG PRESET ONLY*****

Application notes:

The module file is created for a tri-amped cabinet with a HF shelving filter
which can be manipulated by the user. This module file is designed for
near-field applications for up to 3 TFA-600H units.
If using more than 3 cabinets, then increase the high shelf on the EQ page
which is currently set to 0dB gain. 
Or use the preset manager to load preset files into the device.

Technical info:

* Amp Gain is 35.7 dB (LF), 26 dB (MF), 26 dB (HF)
* MaxRMS limiter threshold at +3.3 dBu (LF), +6 dBu (MF), +3 dBu (HF)
* ISVPL threshold at 97.7 Vpk (LF), 61.6 Vpk (MF), 61.6 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +6.3 dBu-pk (LF), +12 dBu-pk (MF), +12 dBu-pk (HF)