Yamaha MY8-LAKE preset suitable for Yamaha Installation series loudspeakers

Application Notes:
IF2112/99 (passive mode) used without a subwoofer

Output Routing:
Ch A: Unused
Ch B: Passive

Limiter Levels:
* When used in the MY8-LAKE, the Analog Output Reference (maximum analog output level) is set to +24 dBu by default
  (which is the case for most of Yamaha consoles). For use with +18 dBu maximum output devices such as DM2000, for example,
  you need to change the Analog Output Reference.
* 26 dB amp gain is assumed.
* MaxPeak Level is set at the MAX power rating.
* MaxRMS Level is 6 dB lower than MaxPeak Level in user level to correspond with NOISE power rating.
* However, the limiter levels should be adjusted according to the amplifiers and your applications.
* E.g. for use with 32 dB amp gain, turn each limiter level 6 dB down.
* Note that the use of a limiter does not provide guaranteed protection of your speakers!
  Please refer to these settings as a starting point for your specific application.
