Adamson's PLM Series preset for Adamson's MH121.5 + Spek-Trix Sub

Application Notes:
     Active Mode
     XOVER frequency 120 Hz

Routing:
     MH121 LF : NL4 1+ 1-
     MH121 HF : NL4 2+ 2-
     SPB : NL8 1+ 1-

Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME