Lake preset for MDC-115S SUB

Application Notes:
     The preset is low-passed at 80 Hz

Routing MDC-115S
     3 outputs 

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
