Lab.gruppen's PLM Series preset suitable for L-Acoustics' KS28 speaker. v5.8

Application notes:
Optimised for CONTOUR configuration

The preset is low-passed at 60 Hz, for use as stand alone sub for K1 and K2 systems. Use the K1SB_X if K1SB is part of the K1 line source or K1SB_X_K2 for K2 line source.

Please be aware of the routing limitations regarding input gain, 
input eq and input delay, when using the channel K1SB 3.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +6 dBu (SUB)
* ISVPL threshold at 115 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +11.5 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk