Lake preset for ADAMSON IS213
========================

Application Notes:
     - Omni-directional
     - No linear phase compensation delay included (add 5.5 ms for linear phase compensation)
     - Low passed at 80 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - IS213
 
Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2
