Lake preset for MDC-2 SUB

Application Notes:
     The preset is low-passed at 80 Hz

Routing MDC3
     3 outputs

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME