*** Tannoy VSX BP ***
___________________________________________

PLM & LM Series preset for Tannoy Bandpass (BP) Subs
VSX 8.2BP, VSX 10BP, VSX 12.2BP
___________________________________________

Application Notes:

This 3 AUX module allows use of the 3 separate Subwoofer
products for combination with suitable Full-Range Cabinets.

The X-over is set to 80Hz for use in combination with Lake/PLM/IPD VX Cut presets.
Maximum of 4 VSX8.2 or VSX10 cabinets in parallel per channel.
Maximum of 2 VSX12.2BP cabinets in parallel per channel.
___________________________________________

Routing:

Any channel can be routed to the required output from this module.
WARNING:: Ensure correct routing before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 1.16 mS
___________________________________________

Fingerprint :	

No
___________________________________________

*** Designed by TCGROUP AET ***


::: Thomas Vestergaard :::
