PLM Series preset for MDC12 in Passive Mode + MDC1

Application Notes:
     Passive Mode
     The preset is High-passed at 100Hz
     FLAT EQ curve for FOH position  
     MDC12 : Maximum 3 cabinets in parallel per channel. 

Routing:
     MDC1 : 1+ 1-
     MDC12 : 1+ 1-
     NL4 connector with Xlink of MDC1 output
     can be used to plug MDC12 using one cable.

Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME