PLM series preset for Juno sub arrayable subwoofer element.

-Application Notes
     1 way Subwoofer element
     No directivity pattern processing
     Low-pass @ 70 Hz
     3 Juno sub elements in parallel per channel

-Routing
     Sub : 1 / 2 / 3 / 4
   
-Technical info
     Amp Gain :  32 dB

-Fingerprint file
    in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
