*** Tannoy cMS3 Series ***
___________________________________________

PLM & LM Series preset for Tannoy CMS3 Series
Products utilised in Passive LOW Z mode or in 100V mode


CMS403DCe, CMS503DC, CMS503DC LP, CMS603DC, CMS803DC, CMS803DCQ
CMS403ICTe, CMS503ICT, CMS503ICT, CMS503ICT LP
___________________________________________

Application Notes:

This 3 AUX module has 3 Processed outputs:

1 = FLAT : Fullrange Settings
2 = CUT  : 120Hz LF Cut (For use either standalone or with Sub)
3 = SUB  : Matched Sub output for use with the above CUT output

This module can be used in combination with CMS801 Sub Module Files
should a different combination other than the one 
supplied be required.
___________________________________________

Routing:

Any channel can be routed to the required output from this module.
WARNING:: Ensure correct routing before use.
___________________________________________      

** Designed by TCGROUP AET ***

::: Thomas Vestergaard :::
