Lake preset for ADAMSON S7p Bi-Amped 70x40
===============================

Application Notes:
     - Fullrange Mode
     - Conventional Crossover
     - Add 6.2 ms of delay for high frequency phase alignment with linear phase presets at the same distance 
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 1
     - Module out 2 - HF: Ch. 2

Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2