Adamson's PLM Series preset for Adamson's SXSUB.

Application Notes:
     The preset is low-passed at 90 Hz 
     Maximum of 2 cabinets per Channel.

Routing:
     SXSUB : 1+ 2- & 2+ 1-
     Need Extra Audio Panel

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME