*** Tannoy VLS ***
___________________________________________

PLM & LM Series preset for Tannoy VLS & VSX 8.2BP
___________________________________________

Application Notes:

Low Impedance Setting on VLS must be active.
Normal EQ curve for standalone and Cut EQ Curve for use with VSX 8.2BP subwoofer.
Maximum of 4 cabinets in parallel per channel.
___________________________________________

Routing:

Any channel can be routed to the required output from this module
WARNING:: Ensure correct routing before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 1.16 mS
___________________________________________

Fingerprint :	

No
___________________________________________

*** Designed by TCGROUP AET ***

::: Thomas Vestergaard :::


