*** TURBOSOUND TQ Series                                     ***
***       V1.2 XP RELEASE                                    ***
*** All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.0.2 ***
*** All MODULES ARE CONTOUR XP FORMAT                        ***
***         README                                           ***
______________________________________________________________________________________________________
LAB GRUPPEN PLM12K44/PLM20K44 & D SERIES L DSP AMPLIFIERS ONLY - LM SERIES PROCESSORS ARE NOT SUITABLE

TQ8/10/12/15 1W PASSIVE XP module for use with TQ15B & TQ18B subs OR stand alone
Pre-aligned for use with TQxxB XP subwoofer Modules in Traditional Mode (pol rev, +1ms on the subwoofer)
if grilles are aligned between TQxx and TQ subwoofer

HR version is for HORN ROTATED - this is important as DSP processing is changed to optimise differing Horn Dispersion

OUTPUTS:  CORRECT OUTPUT PATCHING XP Modules DO NOT REQUIRE MOM (module output mixing) 
instead they use the new MBL (multi-band limiter)

ISVPL profile should be set to universal, From Rev 1.2 ISVPL is optimised from Rev 1.1
______________________________________________________________________________________________________

EQ OVERLAYS:

2 band BLEQ is set at internal crossover points of TQ8/10/12/15 and should be used as a 'tone/level' control. 


Notes:
 
1) do not insert ANY Array Size Compensation overlay


2) DISTANCE EQ (AirEQ) overlay not required

_______________________________________________________________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM / D series L this is already set and locked)

WARNING: Ensure correct routing before use 

_______________________________________________________________________________________________________      

Please read the TQ QSG prior to use 

*** Designed by Music Tribe - APR 2024 ***
http://www.turbosound.com
