EV's PLM Series preset suitable for EV's X-LINE System.

Application Notes:
EV XVLS 4w Mode with 80Hz (LR24) Hi-Pass

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.

EV Rev Number: Version 4 (Standart Preset IIR)
Dolby Lake Rev Number: Version 1.0

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 130 Vpk (LF), 110 Vpk (MF), 84 Vpk (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)