TURBOSOUND's NuQ152 CUT Bi-Amped FIR preset + NuQ118B SUB

This preset is for FOH applications.

As this is an FIR preset, two modules of processing are required (A+B or C+D) and this preset is not compatible with LM series processors.

Application notes:

Channel 1 = NuQ118B SUB
Channel 2 = NuQ152 LF
Channel 3 = NuQ152 HF

HPF on LF channel is at 100Hz for use with NuQ115B

Total Processor Delay is 6.31ms

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at 3.7 dBu (SUB), 3 dBu (LF), -9.3 dBu (HF)
* MaxPeak limiter threshold at 9.7 dBu (SUB), 9 dBu (LF), -3.3 dBu (HF)
* ISVPL threshold at 100 Vpk (SUB), 89 Vpk (LF), 22 Vpk (HF)  

**Designed by MUSIC TRIBE BRANDS Ltd 2019**
