EAW's PLM Series preset for EAW's KF speaker
 
KF650z Tri-amp Full Range

Application Notes:
KF650z is high-passed at 33 Hz with 24 dB Linkwitz-Riley filter for 
full range operation.

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.