Adamson's PLM Series preset for Adamson's Y10.

Application Notes:
     Y10 : LF = Paper Cone Driver 8Ohms
     The preset is high-passed at 90 Hz 
     Maximum 4 cabinets in parallel per amplifier.

Routing:
     LF : 1 & 2
     MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     No

Designed by DV2
Pascal GUILLAUME
     