Lab.gruppen's PLM Series preset suitable for L-Acoustics' KS28 speaker. v5.8

Application notes:
Optimised for THROW configuration with K1

The preset is low-passed at 200 Hz, for use in K1 line source systems. 

Please be aware of the routing limitations regarding input gain, 
input eq and input delay, when using the channel K1SB 3.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +6 dBu (SUB)
* ISVPL threshold at 115 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +11.5 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk