PLM Series preset for MDC-2 SUB

Application Notes:
     CARDIOID MODE FB : Front Back
     The preset is low-passed at 100 Hz 
     Maximum of 1 cabinet per Channel

Routing:
     SUB : 1
     OUTPUT to crosslink SUB2 : 2
     Need to adjust Output routing to choose cardioid FRONT or BACK channel

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME