*** TURBOSOUND MANCHESTER Series                             ***
***       V2.3 XP RELEASE                                    ***
*** All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.0.2 ***
*** All MODULES ARE CONTOUR XP FORMAT                        ***
***         README                                           ***
______________________________________________________________________________________________________
LAB GRUPPEN PLM12K44/PLM20K44 & D SERIES L DSP AMPLIFIERS ONLY - LM SERIES PROCESSORS ARE NOT SUITABLE

THIS MODULE IS FOR THE FRONT SPEAKER IN A 2 ROW INVERTED END FIRE BASS CELL
DISTANCE FROM REAR OF 'FRONT' SUBWOOFER TO FRONT GRILL OF 'REAR' SUBWOOFER IS 44cm

                                      THIS
MODULE     SPACE       MODULE
> REAR     <44CM>      FRONT>  

REAR AND FRONT AMOUNTS OF CABINETS MUST BE EQUAL
EXAMPLE 1+1, 2+2, 3+3
   


MS121 front speaker 44cm XP module for use with MANCHESTER SERIES ARRAY & POINT SOURCE ELEMENTS
Pre-aligned for use with MANCHESTER SERIES ARRAY & POINT SOURCE ELEMENTS

OUTPUTS:  CORRECT OUTPUT PATCHING XP Modules DO NOT REQUIRE MOM (module output mixing) 
instead they use the new MBL (multi-band limiter)

ISVPL profile should be set to Sub/LF for 21" LF 
______________________________________________________________________________________________________

EQ OVERLAYS: NOT REQUIRED
_______________________________________________________________________________________________________
Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM / D series L this is already set and locked)

WARNING: Ensure correct routing before use 

WARNING: V1.1 & V2.3 MODULES ARE NOT DESIGNED TO BE USED TOGETHER IN THE SAME SYSTEM
_______________________________________________________________________________________________________      

Please read the MANCHESTER QSG and Rigging Manual prior to use 

All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.0.2

*** Designed by TURBOSOUND - MAR 2024 ***
http://www.turbosound.com