RM28
Dual 8 inch Coaxial Reference Monitor (Bi-amp)
90 x 60 degree nominal beamwidth

Application Notes:
Use when monitor is placed in vertical orientation.

Technical info:
* Amplifier Gain is set to 32 dB.
* Factory ISVPL Speaker Thresholds and MaxRMS Limiter Thresholds are engaged.