Lab.gruppen's PLM Series preset suitable for L-Acoustics' X8 full range, with optional SB15 sub output. V5.8

Application notes:
The module file is a one-way configuration, high-passed at 50 Hz on output 2. 
SB15 is on output 1. Output 3 is an Aux output.
(The X8 filter is IIR for shortest latency of 1.71 ms.)
Input delay at 2.12ms to match system delay of 3.83 ms.
Delay range is 0 - 20 ms for both enclosures for flexible placement

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +5 dBu (X8), 9 dBu (SB15)
* ISVPL threshold at 124 Vpk (X8), 143 Vpk (SB15)
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +17 dBu-pk (X8), +14 dBu-pk (SB15)

