PLM Series preset for MDC12 in Passive Mode

Application Notes:
     Passive Mode
     Wedge monitor position
     Maximum 3 cabinets in parallel per channel.

Routing:
     MDC12 : 1+ 1-
     

Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME
