Lake preset for ADAMSON PC6
=======================

Application Notes:
     - Low cut at 100 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - FR
     - Module out 2 - FR

Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2
