Lab.gruppen's PLM Series preset suitable for L-Acoustics' dV-DOSC speaker.

Application notes:
Created for the "dV-DOSC 2W 80 LO" application; 
dV-DOSC (80 Hz HPF + LF shelving EQ) normal HF shelving EQ (smooth)
Made to be used with "dVSUB 80 Hz", but can also be used with e.g.
"SB218 80 Hz" or "SB118 80 Hz" provided that the delay and gain is tweaked. 

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +6 dBu (LF), +1 dBu (HF)
* ISVPL threshold at 109.6 Vpk (LF), 61.6 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +11 dBu-pk (LF), +6 dBu-pk (HF)

Fingerprint info:
dV-DOSC v1.0 beta1