Lab.gruppen's PLM Series preset suitable for L-Acoustics' SB15 speaker. v5.8
 
Application notes:
The preset is low-passed at 100 Hz, for use in combination with e.g. 
KARA and K-systems.

In cardioid mode, use an array of four vertically stacked cabinets 
with the bottom cabinet reversed. Route channel SB15C F to 
the upper three cabinets and SB15C R to the bottom cabinet. 
If using several arrays, the distance between each pair must be 
0.6 m (2 ft).
In normal mode, use SB15 100


Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +9 dBu (SUB)
* ISVPL threshold at 143 Vpk (SUB)
* Input delay is set to align with system amp
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +16 dBu-pk 