End user's PLM Series preset suitable for L-Acoustics' KUDO speaker.

Application notes:
Preset for 110 degrees operation and high-passed at 30 Hz.
In use, route channel LF to two separate amplifier outputs, driving one LF driver each.

Created by Norwest Productions Pty. Ltd.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (LF), +7 dBu (MF), +4 dBu (HF)
* MaxPeak limiter threshold at +13 dBu-pk (LF), +12 dBu-pk (MF), +9 dBu-pk (HF)
* ISVPL threshold at 141.0 Vpk (LF), 125.0 Vpk (MF), 90.0 Vpk (HF)

Fingerprint info:
KUDO v1.0b2
Approved ambient temperature range +12 - +50 degrees Celsius