Lab.gruppen's PLM Series preset suitable for L-Acoustics' KS28 speaker. v5.8

Application notes:
The preset is low-passed at 100 Hz, for use in combination with large format line sources, e.g. K1 and K2 systems.

In cardioid mode, use an array of four vertically stacked cabinets 
with the bottom cabinet reversed. Route channel KS28 FRONT to 
the upper three cabinets and KS28 REVERSE to the bottom cabinet. 

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +7 dBu (SUB)
* ISVPL threshold at 137 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +12 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk