Lake XP preset for ADAMSON IS7p 70x40
=======================

Application Notes:
     - Low cut
     - Recommended to use with 100 Hz Subwoofer Presets
     - Linear Phase response matching all E-, S- and IS-Series Line Source and Point Source when positioned in the same distance 
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 1
     - Module out 2 - HF: Ch. 2

Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2