VE = biamped

Two speakers are powered by a single four channel Lab.gruppen PLM amplifier, 
using the integrated Lake active cross-over between LF and MF, 
while passively filtering the MF/HF cross-over point.

With Dynaudio ESOTAR driver technology, M3VE takes over where most other monitor systems give up. 
Attention to detail, underpinned by a 22Hz - 21kHz frequency response and beyond 133dB SPL, 
M3VE leaves no room for desire in terms of resolution, range or power.