*** TURBOSOUND LIVERPOOL TLX Series ***
***       BETA RELEASE              ***
____________________________________________________

TLX215L 1-WAY 80 Hz module

OUTPUTS: Ch1 = TLX215L Sub (80 Hz LPF, inverted polarity)

Pre-aligned for use with TLX84 when processed with
"TLX84 2W 80 Hz" module (3:1 ratio TLX84:TLX215L)
____________________________________________________

EQ OVERLAYS:

- LT COMPENSATION  

Notes:
 
1) insert LT COMPENSATION to maintain tonal balance
consistency when LT or XLT overlays are inserted in
"TLX84 2W 80 Hz" module
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TLX QSG and Rigging Manual prior to use 

*** Designed by Music Group - 16 MAR 2017 ***
http://www.music-group.com/support/