Adamson's PLM Series preset for Adamson's SX18 v5.0

Application Notes:
     Active Mode 3 way
     The preset is high-passed at 80 Hz 
     2 Cabinets per channel

Routing SX18:
     LF : 1+1- 
     MF : 2+2-
     HF : 3+3-

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME
Daniel GRUBAC