*** Turbosound ATHENS TCS Series ***
____________________________________________________

PLM & LM series modules:

TCS62, TCS122/64/94/96, TCS152/64/94/96, TCS110B, TCS212B,TCS115B,TCS218B
____________________________________________________

Application Notes:

GAIN: all modules assume amplifier gain is 35dB.
For PLM this is already set and locked.
____________________________________________________

These models have 1, 2 or 3 processed output channels:
FR = Full Range (1 Channel)
FR + Sub = Full Range and Subwoofer (2 Channels)
Bi-amp Full Range (2 Channels)
Bi-amp + Sub (3 Channels)
Subwoofer (2 Channels)
____________________________________________________

Routing:

Any channel can be routed to the required output
from these modules.

WARNING: Ensure correct routing before use.
____________________________________________________      

*** Designed by Music Group ***

::: Andrew Pardoe 16/01/14 ::::